CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/spect/uxnmr.info
Date         : Tue Oct 25 13:32:45 2022
Release      : TOPSPIN Version 3.2-pl6
Installed in : C:/Bruker/TopSpin3.2
Host         : CZC4033FFL
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU E5-1620 v2 @ 3.70GHz (8 cores at 3691 MHz with Hyperthreading)
User         : nmr
Description  : AVIII HD 600MHz
Location     : Shanghai Jiaorong University Shanghai
System       : Avance III NMR spectrometer
1H-frequency : 600.13 MHz
Order Number : 10121545
Configured in: C:/Bruker/TopSpin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.253
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/03947 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.2 REC-1  AQS RXAD/2 600 Z130588/1280 ECL 00.02
     3   0x34 0xd6   0x1        X  4.1 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/01668 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x32     0        S  2.2 SGU-2  AQS SGU/3 600 (2CH) Z117129/01667 ECL 02.02 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345092_0684 W1345092/0684 ECL 11:
- TCP/IP address = 149.236.99.251
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0684 ECL 11
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2648 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7987 ECL 50
BLA_W1345096_1048 W1345096/1048 ECL 30:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/1048 ECL 30
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/2166 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/8081 ECL 50
LTRX Z109890/00515 ECL 03.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00515 ECL 03.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20161026
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00515 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/02128 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/02426 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - BACS2_H15000-01_532: at TCP/IP address 149.236.99.126


Cryo Controller CRCO: device connected to 149.236.99.253:/dev/tty04

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.4%/0.0deg, reflection meter)
                 PN=Z103205, SN=00506 from 20140221
    Module  2 : 2H
                 PN=Z003473, SN=01302 from 20140211
    Module  3 : XBB19F 2HS
                 PN=Z003506, SN=01508 from 20140312
    Module  4 : 13C
                 PN=Z003524, SN=01000 from 20140304
    Module  5 : 15N
                 PN=Z003530, SN=00784 from 20131212


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/1048 at TCP/IP 149.236.99.250)
SGU1 AUX  output -> input 1 of transmitter 1 (BLAX300 E 6-365MHZ INR W1345092/0684 at TCP/IP 149.236.99.251)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/1048 at TCP/IP 149.236.99.250)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 2 of transmitter 1 (BLAX300 E 6-365MHZ INR W1345092/0684 at TCP/IP 149.236.99.251)
SGU3 AUX  output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/1048 at TCP/IP 149.236.99.250)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX300 E 6-365MHZ INR W1345092/0684 at TCP/IP 149.236.99.251) amplifier X-300W uses blanking 4
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/1048 at TCP/IP 149.236.99.250) amplifier 1H-100W uses blanking 2
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/1048 at TCP/IP 149.236.99.250) amplifier X-300W uses blanking 1
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/1048 at TCP/IP 149.236.99.250) amplifier 2H-150W uses blanking 6
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00515 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

