CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl6/conf/instr/MDCL700/uxnmr.info
Date         : Thu Feb  2 10:46:05 2017
Release      : TopSpin 3.5 pl 6
Installed in : /opt/topspin3.5pl6
Host         : pansy
OS           : CentOS release 5.11 (Final)
CPU          : Intel(R) Core(TM)2 Duo CPU E8300 @ 2.83GHz (2 cores at 1998 MHz)
User         : IconStart (Icon Start)
System       : Avance III 700 NMR spectrometer
1H-frequency : 700.17 MHz
Description  : Avance III 700
Location     : MDCL-2335
Bruker Order : CH005509
Configured in: pansy:/opt/topspin3.5pl6/conf/instr/MDCL700

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.250
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01552 ECL 05.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2
DRU2: AQS DRU-E Z102520/01553 ECL 05.00
- TCP/IP address = 149.236.99.88
- Firmware Version = 151014

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AW  R  4.5 REC-1  AQS RXAD1000 Z102118/250 ECL 04.05
     3   0x34 0xc1   0x1        X  2.2 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x29   0x8    AE  S  3.4 SGU-1  AQS SGU/2 1000 Z103082/00518 ECL 03.04 FPGA-Vs=AF
     6   0x11 0x52   0x4    AW  R  4.4 REC-2  AQS RXAD1000 Z102118/208 ECL 04.04
     7   0x25 0x29   0x8    AE  S  3.4 SGU-2  AQS SGU/2 1000 Z103082/00520 ECL 03.04 FPGA-Vs=AF
     8   0x26 0x29   0x8    AE  S  3.4 SGU-3  AQS SGU/2 1000 Z103082/00521 ECL 03.04 FPGA-Vs=AF
     9   0x27 0x29   0x8    AE  S  3.4 SGU-4  AQS SGU/2 1000 Z103082/00522 ECL 03.04 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0119 W1345097/0119 ECL 1:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0119 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0661 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00781 ECL 03
BLA_W1345092_0283 W1345092/0283 ECL 1:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0283 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0885 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00708 ECL 03

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: not available
- Lock: installed

Bruker Automatic Changer: device connected to 149.236.99.250:/dev/tty04
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 5 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.250:/dev/tty05

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 149.236.99.55

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AO
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003463, SN=00641 from 20090306
    Module  2 : XBB19F 2HS
                PN=Z003507, SN=00173 from 20090311
    Module  3 : 2H
                PN=Z003474, SN=00130 from 20081124
    Module  4 : XBB19F 2HS
                PN=Z003507, SN=00172 from 20090311



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0119 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0119 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0283 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0119 at TCP/IP 149.236.99.253)
SGU4 NORM output -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0283 at TCP/IP 149.236.99.252)
SGU4 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0119 at TCP/IP 149.236.99.253)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0119 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking

transmitter 2 = BLAX300 E 6-365MHZ INR W1345092/0283 at TCP/IP 149.236.99.252:
- amplifier X-300W uses blanking 3


